Valve ED has flow rate=0; tunnels lead to valves PS, AW
Valve SI has flow rate=0; tunnels lead to valves AA, HX
Valve LX has flow rate=22; tunnels lead to valves DY, YH
Valve CR has flow rate=0; tunnels lead to valves BE, HX
Valve BI has flow rate=0; tunnels lead to valves GC, AY
Valve PB has flow rate=4; tunnels lead to valves IX, YG, RI, KR, BV
Valve YY has flow rate=0; tunnels lead to valves PH, GJ
Valve PH has flow rate=11; tunnels lead to valves YY, VE, ZG, MM
Valve DY has flow rate=0; tunnels lead to valves LX, AW
Valve SD has flow rate=0; tunnels lead to valves AY, EC
Valve SV has flow rate=24; tunnels lead to valves CC, GF
Valve RL has flow rate=0; tunnels lead to valves OW, IN
Valve GF has flow rate=0; tunnels lead to valves RQ, SV
Valve BE has flow rate=5; tunnels lead to valves CR, JC, MF, IT
Valve PR has flow rate=0; tunnels lead to valves BV, GJ
Valve AW has flow rate=21; tunnels lead to valves VE, DY, TR, ED
Valve FY has flow rate=17; tunnels lead to valves GG, KJ
Valve GC has flow rate=0; tunnels lead to valves BI, GJ
Valve RI has flow rate=0; tunnels lead to valves PB, AY
Valve RQ has flow rate=0; tunnels lead to valves HH, GF
Valve IT has flow rate=0; tunnels lead to valves MZ, BE
Valve XG has flow rate=0; tunnels lead to valves BL, AA
Valve MK has flow rate=0; tunnels lead to valves HX, DV
Valve IX has flow rate=0; tunnels lead to valves PB, JC
Valve BV has flow rate=0; tunnels lead to valves PR, PB
Valve TR has flow rate=0; tunnels lead to valves CD, AW
Valve PS has flow rate=0; tunnels lead to valves ED, AY
Valve HH has flow rate=12; tunnels lead to valves RQ, NL, ZQ
Valve AA has flow rate=0; tunnels lead to valves KR, SI, XG, EC, ZG
Valve FT has flow rate=0; tunnels lead to valves IN, YH
Valve YG has flow rate=0; tunnels lead to valves PB, HX
Valve HX has flow rate=14; tunnels lead to valves MK, ZQ, YG, SI, CR
Valve DV has flow rate=0; tunnels lead to valves MK, QR
Valve GJ has flow rate=3; tunnels lead to valves PR, CD, YY, GC, BL
Valve BL has flow rate=0; tunnels lead to valves GJ, XG
Valve CD has flow rate=0; tunnels lead to valves TR, GJ
Valve GG has flow rate=0; tunnels lead to valves FY, NL
Valve JC has flow rate=0; tunnels lead to valves IX, BE
Valve JN has flow rate=0; tunnels lead to valves OW, QR
Valve RM has flow rate=18; tunnel leads to valve KJ
Valve NL has flow rate=0; tunnels lead to valves GG, HH
Valve QR has flow rate=20; tunnels lead to valves CC, DV, PN, JN
Valve ZG has flow rate=0; tunnels lead to valves AA, PH
Valve AY has flow rate=6; tunnels lead to valves RI, PS, SD, BI, MM
Valve VE has flow rate=0; tunnels lead to valves PH, AW
Valve OW has flow rate=25; tunnels lead to valves MZ, RL, JN
Valve MM has flow rate=0; tunnels lead to valves AY, PH
Valve KJ has flow rate=0; tunnels lead to valves RM, FY
Valve MF has flow rate=0; tunnels lead to valves BE, PN
Valve YH has flow rate=0; tunnels lead to valves LX, FT
Valve ZQ has flow rate=0; tunnels lead to valves HX, HH
Valve KR has flow rate=0; tunnels lead to valves AA, PB
Valve PN has flow rate=0; tunnels lead to valves MF, QR
Valve CC has flow rate=0; tunnels lead to valves SV, QR
Valve MZ has flow rate=0; tunnels lead to valves OW, IT
Valve EC has flow rate=0; tunnels lead to valves SD, AA
Valve IN has flow rate=16; tunnels lead to valves RL, FT
